The Eleksmana uses an Arduino Nano board with an ATMega328p processor.

In the Arduino upload land it uses the old ATMega328p bootloader!

To use the Eleksmakeer software we need to load the ELEKSROM firmware and then run ELEKSCAM (Make sure you click the install driver button when the GUI is open to install the driver)

NOTE: Make sure the button is on on the device!

Follow the instructions here to make sure everything works.

https://cadduino.wordpress.com/2013/11/18/testing-grbl-in-arduino-board-without-the-motors/